PHILIPS / SIMOCO FM1100 STANDARD HEAD 2 METRE PROGRAM

CHANNELS 00 TO 07 FROM 144.600 TO 144.775 IN 25KHZ STEPS

08 TO 23 IN 25KHZ STEPS CHANNEL NUMBERS EQUATE TO S NUMBERS

24 T0 55 IN 12KHZ STEPS EVEN NUMBERS REPEATER CHANNELS ODD NUMBERS REVERSE REPEATER CHANNELS IE: 24 = R0 25 = REVERSE R0

56 = 145.8 INTERNATIONAL SPACE STATION

57 TO 71 144.8 TO 144.975 IN 12.5 KHZ STEPS

72 TO 75 CHANNELS USED IN NORTHERN IRELAND FOR ECHOLINK

STARTING CHANNEL LAST USED CHANNEL

FIRST FUNCTION BUTTON SELECTS LOW POWER OF 1 WATT

SECOND FUNCTION BUTTON OPENS SQUELCH

THIRD BUTTON TOGGLES BACKLIGHT ON / OFF

FOURTH BUTTON SHOWS CTCSS NUMBER

FIFTH BUTTON TOGGLES CTCSS OFF AND ON

SEVENTH FUNCTION BUTTON DECREMENTS CHANNELS

EIGHTH FUNCTION BUTTON INCREMENTS CHANNELS

PM ME FOR FURTHER DETAILS AS TO GETTING YOUR FIRMWARE EPROM CHIP 27C512 AND EEPROM CHIP 24C16 TO ME.