PHILIPS / SIMOCO FM1100 STANDARD HEAD 4 METRE PROGRAM

CHANNELS 00 TO 41 FROM 70.00 TO 70.50 IN 25KHZ STEPS.

AND CHANNEL 42 GIVING SCAN FROM 36 TO 41.

STARTING CHANNEL 36 70.45.

FIRST FUNCTION BUTTON SELECTS LOW POWER OF 1 WATT

SECOND FUNCTION BUTTON OPENS SQUELCH

THIRD BUTTON TOGGLES BACKLIGHT ON / OFF

SEVENTH FUNCTION BUTTON DECREMENTS CHANNELS

EIGHTH FUNCTION BUTTON INCREMENTS CHANNELS

PM ME FOR FURTHER DETAILS AS TO GETTING YOUR FIRMWARE EPROM CHIP 27C512 AND EEPROM CHIP 24C16 TO ME.